400w LED三合一参数
输入电压:AC110v - 240 v / 50-60HZ
光源规格400W
光源寿命:20000小时
流明照度: 5米120000 lm
额定功率:430 w
通道模式:23ch
水平扫描:540度(16位精密扫描)电子纠错
垂直扫描:270度(16位精密扫描)电子纠错
调光系统:0-100%线性调节
聚焦系统: 从4米到50米线性调节
雾化系统: 1个独立雾化效果，光斑柔和自然
放大角度: 4-35度
高速频闪: 0-30次/秒。调速频闪效果可调。斯特罗布宏函数
颜色:8色+白光,半色功能
调色系统:线性CMY+CTO调色系统。
固定模式:12个固定模式+白光
旋转图案:7个玻璃图案，每个玻璃图案可独立正反转
棱镜系统:标准单六排棱镜和8棱镜，每个棱镜可独立正反向
宏功能:控制台复位功能、自走模式、主从模式
显示方式:液晶显示，按键+触摸双操作模式
控制信号:国际标准DMX512。具有RDM功能，可进行软件在线升级，拨打地址码
冷却方式:采用轴流风机加强冷却
安全装置:设有电子温控过热保护，当过热系统失效时，电子温控自动断电保护
外观材料:耐高温塑料
工作环境:-20度- 40度
保护级别:IP20
产品净重:22.5KG
产品尺寸:38*27*65CM (L*W*H)






Input voltage: AC110V-240V/50-60HZ
Light source specification: led 400W
Light source life: 20000 hours
[bookmark: _GoBack]Lumen illuminance: 5 meters 120,000 lm
Rated power: 430W
Channel mode: 23 channels
Horizontal scan: 540 degrees (16bit precision scan) electronic error correction
Vertical scanning: 270 degrees (16bit precision scanning) electronic error correction
Dimming system: 0-100% linear adjustment
Focusing system: linear adjustment from 4 meters to 50 meters
Frost system: 1 independent frost effect, soft and natural light spot
Zoom angle: 4-35 degrees
High-speed strobe: 0-30 times/sec. Adjustable speed strobe effect. Strobe macro function
Color: 8colors + white light. Color half-color function
Color mixing system: linear CMY+CTO color mixing system.
Fixed patterns: 12 fixed patterns + white light
Rotating pattern: 7 glass patterns, each glass pattern can be independently forward and reverse
Prism system: standard 6 facet prism and 8 facet prism, each prism can be independently forward and reverse
Macro function: console reset function, self-propelled mode, master-slave mode
Display mode: LCD display, key + touch dual operation mode
Control signal: International standard DMX512. With RDM function, online software upgrade is available, dial address code
Cooling method: Adopt axial fan to enhance cooling
Safety device: with electronic temperature control overheating protection, electronic temperature control automatic power-off protection when the overheating system fails
Appearance material: high temperature resistant plastic
Working environment: -20 degrees - 40 degrees
Protection level: IP20
Product net weight: 22.5KG
Product size: 38*27*65CM (L*W*H)

