Input Voltage: AC 100-240V, 50-60Hz

Power Consumption: 500W

Light Source: 19 x 15W RGBW LEDs

Color Temperature: 2500-8000K (linear adjustment)

Control: DMX512 / Master-Slave / Auto-run / Sound-activated

Electronic Zoom Beam Angle: 4°-60°

Modes: Wash, Beam, Graphic, Effect

(Vortex, Kaleidoscope, "Wasp Waist")

Front lens disc supports bidirectional continuous rotation

0-100% linear electronic dimming

Strobe: 0-25 flashes/second

RGBW infinite color mixing system

Channels: 21/23/35/78/92/97/99 channels (7 channel modes)

Operating Temperature: -25°C to 40°C

Lifespan: 50,000 hours

Movement Range: Pan 540° + 16-bit fine-tuning;

Tilt 270° + 16-bit

IP Rating: IP20 (indoor use)

Packaging Dimensions: 494 x 358 x 253 mm

Net Weight: 15 kg

输入电压:AC100-240V,50-60Hz

消耗功率:500W

光源:19颗15W RGBW LED

色温：2500-8000K 可线性调节

控制:DMX512/主从机/自走/声控

电子调焦光束角度:4°-60°

染色，光束，图像，效果模式

（漩涡，万花筒，小蛮腰）

前置镜盘可双向地无极旋转

0-100%线性电子调光

频闪: 0-25次/秒

RGBW无极混色系统

通道:21/23/35/78/92/97/99通道，7种通道模式

工作温度:-25°C-40°C

使用寿命:5,0000小时

移动范围:水平540°+16bit微调,

         垂直:270°+16bit

防水等级:IP20(室内使用)

包装尺寸:494*358*253mm

净重:15kg

